{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["default","downcodes2","downcodes3","downcodes4","downcodes5","downcodes6","downcodes7","category","category2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":15,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"default","index":0,"n_rows":32,"n_cols":2,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Code","Reason"]
["INT","INTERMITTENT FLOW"]
["WO","WORK OVER"]
["PBUP","PRESSURE BUILD UP"]
["DHP","DOWN HOLE PROBLEMS"]
["HLP","HIGH LINE PRESSURE"]
["COMP","COMPRESSOR (UNSCHEDULED)"]
["CMPS","COMPRESSOR (SCHEDULED)"]
["CNTR","CONTROLLER MALFUNCTION"]
["CONU","CONSTRUCTION (UNSCHEDULED"]
["CONS","CONSTRUCTION (SCHEDULED)"]
["EQRG","REGULATOR FREEZE/FAILURE"]
["MECH","MECHANICAL (UNSCHEDULED)"]
["MECS","MECHANICAL (SCHEDULED)"]
["STOW","SHUT IN TEST OTHER WELL"]
["SIS","SHUT IN AFTER SWAB"]
["STFU","SHUT IN TANK FULL (UNSCHE)"]
["STF","SHUT IN TANK FULL (SCHEDU)"]
["WEA","WEATHER"]
["WLU","WELL LOADED UP"]
["WSU","WELL SANDED UP"]
["DEP","DEPLETED"]
["MTRF","METER FREEZE"]
["MTRL","METER FAIL"]
["MKT","MARKET DEMAND"]
["PLF","PIPELINE FREEZE"]
["PLR","PIPELINE REQUEST"]
["REG","REGULATORY"]
["PLL","PIPELINE LEAK"]
["IP","INITIAL PRODUCTION"]
["GLK","GAS LOCK"]
["OTH","OTHER"]

{"sheet":"downcodes2","index":1,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Code","Reason"]
["DHP","Downhole Problems"]
["ELEQ","Electrical Equip"]
["ELPW","Electrical Power - 3rd Party"]
["MECH","Mechanical"]
["PLAN","Planned"]
["PBUP","Pressure Build Up"]
["INT","Prod Intermittent"]
["REG","Regulatory"]
["SMTL","Sales Meter / Tank"]
["SMT3","Sales Meter / Tank - 3rd Party"]
["WEA","Weather"]
["WLU","Well Loaded"]
["WO","Workover"]
["UNEC","Uneconomic to Produce"]

{"sheet":"downcodes3","index":2,"n_rows":29,"n_cols":2,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Code","Reason"]
["$LD","SOLD/TRANSFERRED"]
["BAT","WO BATTERY"]
["BLT","CHANGE BELTS "]
["DRG","DRILLING"]
["ELC","ELECTRICAL PROBLEMS"]
["EQP","WO EQUIPMENT"]
["FLL","WO/CONNECT FLOWLINE"]
["FLW","STOP FLOWING"]
["GBX","GEAR BOX PROBLEMS"]
["HTR","HEATER TREATER PROBLEMS"]
["MTR","MOTOR PROBLEMS"]
["ND ","NOT DRILLED "]
["PA ","PLUGGED AND ABONDONED"]
["PFN","PARAFFIN PROBLEMS"]
["PLG","PLUNGER PROBLEMS/SWD"]
["PMP","BAD PUMP/CHANGE PUMP"]
["PU ","PUMPING UNIT DOWN"]
["RCP","RECOMPLETION"]
["ROD","RODS PARTED"]
["SB ","STUFFING BOX LEAK"]
["SI ","SHUT-IN"]
["SWD","SWD DOWN"]
["TA ","TEMPORARILY ABANDONED"]
["TBG","HOLE/SPLIT IN TUBING"]
["TNK","TANKS FULL"]
["WFM","WEATHER/FORCE MAJOR"]
["WO ","WORKOVER"]
["XXX","WELL STATUS REASON CODE"]

{"sheet":"downcodes4","index":3,"n_rows":60,"n_cols":2,"rows_kept":60,"cut":false,"hidden":false,"merged":[]}
["Code","Reason"]
["AC ","Acid Job"]
["AR ","Allowable Restriction"]
["CD ","Compressor Down "]
["CFG","Compressor Down-Fuel Gas"]
["CLL","Compressor Down-Liq Level"]
["COP","Compressor Down-Oil Pres"]
["CR ","Compressor Repair"]
["CWT","Compressor Down-Wtr Temp"]
["CF ","Choke Froze"]
["CP ","Changed Plate"]
["CS ","Clock Stop"]
["DHP","Down Hole Problems"]
["CT ","Chemical Treatment"]
["ET ","Engine Trouble"]
["EO ","Elect Off"]
["EP ","Equipment Problems"]
["GO ","Gas Off"]
["GMR","Gas Meter Reset"]
["HD ","High Disch"]
["LF ","Line Freeze"]
["LMR","Lact Meter Reset"]
["LUW","Loading Up-Water"]
["MP","Mechanical Problems"]
["NC ","Not Capable(vlv open)"]
["NP ","Negative Production"]
["OP ","Over Produced"]
["ODP","Other Downhole Prob"]
["OTH","Other"]
["PRO","Prorated"]
["PO ","Pump Off"]
["PC ","Pipeline Capacity"]
["PP ","Periodic Production"]
["PBS","Purch-Bal Split Conn"]
["PLB","Purch-Line Break"]
["PNC","Purch-No Contract"]
["PHP","Purch-High Line Pres"]
["PMO","Purch-Mrkt Out"]
["PB ","Pressure Buildup"]
["R  ","Resting"]
["REG","Regulatory"]
["RP ","Rod Part"]
["RW ","Reworking"]
["SOF","SI for Offset Frac"]
["SE ","Surface Equipment"]
["ST ","State Test"]
["SW ","Swabbing"]
["TWE","Testing Well-Eval"]
["T  ","Treating"]
["TJ ","Tubing Job"]
["TMR","Transfer Meter Reset"]
["TR ","Tank Room"]
["U  ","Unknown"]
["V  ","Venting"]
["WEA","Weather"]
["WLU","Well Loaded Up"]
["WSU","Well Sanded Up"]
["WOO","Waiting On Orders"]
["WOP","W/O Pipeline Conn"]
["WS ","Well Service-Workover"]

{"sheet":"downcodes5","index":4,"n_rows":24,"n_cols":3,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Code","Reason","Mid-Con Energy"]
["C1","Compressor"]
[]
["D1","Pumped Off - Downhole"]
["D2","Work Over - Downhole"]
["D3","Rod Part - Downhole"]
["D4","Tubing Failure - Downhole"]
["D5","Pump change - Downhole"]
["D6","Pumping Unit - Downhole"]
["D7","ESP Failure - Downhole"]
["D8","Other - Downhole"]
[]
["S1","Inj Pump Prob - Surface"]
["S2","Inject Pump Maint - Surface"]
["S3","Wtr Dump Prob - Surface"]
["S4","Tank - Surface"]
["S5","Fire - Surface"]
["S6","Electrical - Surface"]
["S7","Weather - Surface"]
["S8","Pumping Unit - Surface"]
["S9","Heater Treater - Surface"]
["S10","Flowline - Surface"]
["S11","Tnk full Purchaser - Surface"]
["S12","Other - Surface"]

{"sheet":"downcodes6","index":5,"n_rows":33,"n_cols":3,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["Code","Reason","RKI"]
["PLL","CNGP PIPELINE LEAK"]
["CMPS","COMPRESSOR (SCHEDULED)"]
["COMP","COMPRESSOR (UNSCHEDULED)"]
["CONS","CONSTRUCTION (SCHEDULED)"]
["CONU","CONSTRUCTION (UNSCHEDULED"]
["CNTR","CONTROLLER MALFUNCTION"]
["DEP","DEPLETED"]
["DHP","DOWN HOLE PROBLEMS"]
["GLK","GAS LOCK"]
["HLP","HIGH LINE PRESSURE"]
["IP","INITIAL PRODUCTION"]
["INT","INTERMITTENT FLOW"]
["MKT","MARKET DEMAND"]
["MECS","MECHANICAL (SCHEDULED)"]
["MECH","MECHANICAL (UNSCHEDULED)"]
["MTRL","METER FAIL"]
["MTRF","METER FREEZE"]
["NLL","NEGATIVE LIQUID LEVEL"]
["OTH","OTHER"]
["PLF","PIPELINE FREEZE"]
["PLR","PIPELINE REQUEST"]
["PBUP","PRESSURE BUILD UP"]
["EQRG","REGULATOR FREEZE/FAILURE"]
["REG","REGULATORY"]
["SIS","SHUT IN AFTER SWAB"]
["STF","SHUT IN TANK FULL (SCHEDU)"]
["STFU","SHUT IN TANK FULL (UNSCHE)"]
["STOW","SHUT IN TEST OTHER WELL"]
["WEA","WEATHER"]
["WLU","WELL LOADED UP"]
["WSU","WELL SANDED UP"]
["WO","WORK OVER"]

{"sheet":"downcodes7","index":6,"n_rows":29,"n_cols":3,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Code","Reason","Strata"]
["PA","PLUGGED AND ABONDONED"]
["PFN","PARAFFIN PROBLEMS"]
["PLG","PLUNGER PROBLEMS/SWD"]
["PMP","BAD PUMP/CHANGE PUMP"]
["PU","PUMPING UNIT DOWN"]
["RCP","RECOMPLETION"]
["ROD","RODS PARTED"]
["SB","STUFFING BOX LEAK"]
["SI","SHUT-IN"]
["SWD","SWD DOWN"]
["TA","TEMPORARILY ABANDONED"]
["TBG","HOLE/SPLIT IN TUBING"]
["$LD","SOLD/TRANSFERRED"]
["BAT","WO BATTERY"]
["BLT","CHANGE BELTS "]
["DRG","DRILLING"]
["ELC","ELECTRICAL PROBLEMS"]
["EQP","WO EQUIPMENT"]
["FLL","WO/CONNECT FLOWLINE"]
["FLW","STOP FLOWING"]
["GBX","GEAR BOX PROBLEMS"]
["HTR","HEATER TREATER PROBLEMS"]
["MTR","MOTOR PROBLEMS"]
["ND","NOT DRILLED "]
["TNK","TANKS FULL"]
["WFM","WEATHER/FORCE MAJOR"]
["WO","WORKOVER"]
["XXX","WELL STATUS REASON CODE"]

{"sheet":"category","index":7,"n_rows":64,"n_cols":4,"rows_kept":64,"cut":false,"hidden":false,"merged":[]}
["Code","LookupType","Reason","New Dominion"]
["DHP","Downtime Code","Down Hole Problems"]
["MECH","Downtime Code","Mechanical"]
["PBUP ","Downtime Code","Pressure Build Up"]
["WO","Downtime Code","Work over"]
["SMTR","Downtime Code","Sales Meter"]
["WEA","Downtime Code","Weather"]
["UEP","Downtime Code","Uneconomic To Produce"]
["Lookup2"]
["DE","DHP","Down For Evaluation"]
["RPRT","DHP","Rod Part"]
["HTBG","DHP","Hole in Tubing"]
["HCSG","DHP","Hole in Casing"]
["PUMP","DHP","Pump Change or pump issues"]
["PLGR","DHP","Plunger issues"]
["ESP","DHP","Electrical Sub Pump Failure"]
["ESP-UL","DHP","Electrical Sub Pump Under load"]
["ESP-OL","DHP","Electrical Sub Pump Over load"]
["ESP-FUSE","DHP","Electrical Sub Pump Fuse Blown"]
["UNKN","DHP","Unknown"]
["CON","MECH","Construction or roustabout "]
["CTRB","MECH","Control Box/Panel"]
["COMP","MECH","Compressor Repair"]
["PU","MECH","Pumping Unit Repair"]
["MTR","MECH","Electric Motor Repair"]
["ENG","MECH","Gas Engine Repair"]
["ELEC","MECH","Electrical issues"]
["FLOL","MECH","Lease Flow line Failure"]
["PARF","MECH","Shut-in Paraffin Problems"]
["SWPR","MECH","SW Transfer Pump Repair"]
["BT","MECH","Bubble Tower Repairs"]
["SWD","MECH","Saltwater Disposal Down"]
["PER","MECH","Production Equipment Repair"]
["PM","MECH","Pipeline Maintenance"]
["WLU","PBUP","Well Loaded Up"]
["TEST","PBUP","Test Pressure Build Up"]
["PLMT","PBUP","Plunger Missed Trip"]
["TRMT","PBUP","Treated Well"]
["STEST/REG","PBUP","Shut-in Regulatory Testing/State Test"]
["INT","PBUP","Time Clock Flow or Pumped Intermittently"]
["MIT","PBUP","Mechanical Integrity Test / OCC"]
["PUDR","PBUP","Pumping unit down on Rotation"]
["WROH","WO","Work Over Rig on Hole"]
["SOH","WO","Swab Unit on Hole"]
["WL","WO","Wire Line work"]
["PLM","WO","Plunger Lift Maintenance"]
["CTBG","WO","Coil Tubing"]
["WOO","WO","Waiting On Orders"]
["PLR","SMTR","Pipeline Request - Incl Pipeline Leaks"]
["HLP","SMTR","High Line Pressure"]
["HO2","SMTR","High Oxygen"]
["H2S","SMTR","High H2S"]
["POS","SMTR","Production out of Purchaser Spec"]
["LPR","SMTR","Pipeline Failure-Not 3rd Party"]
["VNTG","SMTR","Venting Gas"]
["MTRF","WEA","Sales Meter Freeze"]
["PLF","WEA","Pipeline Freeze"]
["RGF","WEA","Regulator or Valve Freeze"]
["UTRW","WEA","Unable to Reach Well"]
["LTGS","WEA","Lightning Strike"]
["ICST","WEA","Ice or Snow Storm"]
["SURF","WEA","Surface Equip Freeze"]
["THNDS","WEA","Thunderstorm"]
["HOE","UEP","High Operating Expenses"]

{"sheet":"category2","index":8,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[[0,4,0,5],[0,0,0,1],[0,2,0,3]]}
["CODE",null,"SUB - CATEGORY",null,"REASON",null,"Linn Energy"]
[1,"DOWN HOLE PROBLEMS"]
[null,"PRT","A","ROD PART",null,"PROBLEMS WITH RODS, POLISHED ROD, SINKER BARS,ETC"]
[null,"TBG","B","HOLE IN TUBING",null,"PROBLEMS WITH TUBING, COUPLINGS, SEALS, ETC"]
[null,"CSG","C","HOLE IN CASING",null,"PROBLEMS WITH CASING, LEAK, COLLAPSE, SPLIT, ETC"]
[null,"PMP","D","PUMP CHANGE OR PUMP ISSUES",null,"PROBLEMS WITH INSERT OR TUBING PUMP"]
[null,"PLR","E","PLUNGER ISSUES",null,"PROBLEMS WITH PLUNGER / INTERMITTER CONTROLLER"]
[null,"ESP","F","ELECT SUB PUMP FAILURE",null,"PROBLEMS WITH SUB PUMP"]
[null,"OTH","G","OTHER DOWNHOLE PROBLEMS",null,"MISC DOWNHOLE PROBLEMS, SANDED-UP, SCALED-UP, TOOLS STUCK IN HOLE, SCSSV FAILURE, UNKNOWN"]
[]
[2,"MECHANICAL"]
[null,"CON","A","CONSTRUCTION OR ROUSTABOUT",null,"DOWNTIME CAUSED BY ANY TYPE OF CONSTRUCTION OR EQUIPMENT REPAIR"]
[null,"CTR","B","CONTROL BOX",null,"PROBLEMS WITH PLUNGER,  INTERMITTER,  OR  CONTROLLER"]
[null,"CMP","C","COMPRESSOR",null,"ANY DOWNTIME CAUSED BY THE COMPRESSOR (Sched or UnSched)"]
[null,"PU","D","PUMPING UNIT",null,"PROBLEMS WITH PUMPING UNIT FRAME, GEARBOX, BASE, etc"]
[null,"MTR","E","ELECTIC MOTOR",null,"PROBLEMS WITH ELECTRIC MOTOR OR WIRING"]
[null,"ENG","F","GAS ENGINE",null,"PROBLEMS WITH GAS ENGINE, FUEL, BELTS, ETC"]
[null,"ENV","G","ENVIRONEMENTAL POT OR SWITCH",null,"DOWNTIME CAUSED BY PUMPING UNIT STUFFING BOX ENVIRONMENTAL EQUIPMENT"]
[null,"ELE","H","ELECTRICAL ISSUES",null,"PROBLEMS WITH ONSITE ELECTRIC WIRING OR POWER"]
[null,"FLO","I","LEASE FLOWLINE FAILURE",null,"PROBLEMS WITH LINN FLOWLINE OR GATHERING SYSTEM - NOT 3RD PARTY PL"]
[null,"PAR","J","PARAFFIN PROBLEMS (SURF OR SUBSURF)",null,"PROBLEMS WITH PARAFFIN BUILDUP IN PERFS, TUBING, CASING, FLOWLINE, EQUIPMENT, TANKS, ETC"]
[null,"EPR","K","ELECTRIC PROVIDER OUTAGE",null,"PROBLEMS WITH ELECTRIC POWER SYSTEM OR 3RD PARTY PROVIDER"]
[null,"MOT","L","OTHER MECHANICAL PROBLEMS",null,"MISC MECHANICAL PROBLEMS"]
[]
[3,"PRESSURE BUILD-UP"]
[null,"WLU","A","WELL LOADED-UP",null,"SHUT-IN TO BUILD-UP PRESSURE TO UNLOAD"]
[null,"TES","B","TEST PRESSURE BUILD-UP",null,"SHUT-IN TO OBTAIN BHP OR FLOWTEST  - NOT REG OR STATE TESTING"]
[null,"PLT","C","PLUNGER MISSED TRIP",null,"SHUT-IN DUE TO PLUNGER MALFUNCTION, ETC"]
[null,"TRT","D","TREATED WELL",null,"SHUT-IN TO CHEMICALLY TREAT WELL,  ALLOW CHEMICAL TO FALL,  UNLOAD FLUIDS AFTER TREAT, ETC"]
[null,"REG","E","SHUT-IN REG TESTING / STATE TEST",null,"SHUT-IN REGULATORY TESTING"]
[null,"INT","F","FLOW OR PUMPED INTERMITTENTLY",null,"PERIODIC PRODUCTION;  FLOWS ON INTERMITTENT BASIS "]
[]
[4,"WORKOVER"]
[null,"WOR","A","WORKOVER RIG ON HOLE",null,"DOWNTIME FOR ALL WORKOVER ACTIVITIES"]
[null,"SWA","B","SWAB UNIT ON HOLE",null,"DOWNTIME WHILE SWABBING UNIT ON WELL OR DIRECTLY AFTER LEAVING WELL - PRESS BUILD-UP AFTER SWABBING"]
[null,"WLU","C","WIRELINE UNIT ON HOLE",null,"DOWNTIME WHILE PERFORMING WIRELINE WORK ON WELL"]
[null,"PLM","D","PLUNGER LIFT MAINTENANCE",null,"DOWNTIME WHILE WORKING ON PLUNGER, LUBRICATOR, CONTROLLER, ETC"]
[null,"CTU","E","COIL TUBING UNIT ON HOLE",null,"DOWNTIME WHILE COILED TBG UNIT ON WELL OR DIRECTLY AFTER LEAVING WELL - PRESS BUILD-UP AFTER JETTING"]
[]
[5,"SALES METER"]
[null,"PLR","A","PIPELINE REQUEST - INCL PL LEAKS",null,"DOWNTIME CAUSED BY PURCHASER OR TRANSPORTER,  PIPELINE PROBLEMS, LEAKS, PLANT PROBLEMS, ETC "]
[null,"HLP","B","HIGH LINE PRESSURE",null,"DOWNTIME CAUSED BY PURCHASER HIGH LINE PRESSURE"]
[null,"HO2","C","HIGH OXYGEN",null,"PRODUCTION OUT OF PURCHASER SPEC (HIGH O2)"]
[null,"POS","D","PRODUCTION OUT OF PURCHASER SPEC",null,"PRODUCTION OUT OF PURCHASER SPEC (HIGH H2S,  CO2,  H2O,  BTU,  ETC)"]
[null,"LPR","E","LINN PIPELINE FAILURE - NOT 3RD PARTY",null,"LINN PIPELINE FAILURE – NOT 3RD PARTY PIPELINE"]
[null,"MKT","F","LINN MRKTG DEPT INITIATED SHUT-IN",null,"LINN MRKTG DEPT INITIATED SHUT-IN DUE TO MARKETING CONDITIONS - NOT 3RD PARTY"]
[]
[6,"WEATHER"]
[null,"SMF","A","SALES METER FREEZE",null,"PROBLEMS WITH SALES METER MEASURING GAS FLOW - HYDRATES, ETC"]
[null,"PLF","B","PIPELINE FREEZE",null,"PROBLEMS WITH PIPELINE - HYDRATES, ETC"]
[null,"RGF","C","REGULATOR OR VALVE FREEZE",null,"PROBLEMS WITH REGULATORS, BACK-PRESSURE VALVES, FLOW CONTROLLERS, ETC"]
[null,"WEA","D","DANGEROUS WEATHER CONDITIONS",null,"ALL WEATHER RELATED REASONS - HURRICANE, TORNADO, SNOW, RAIN, FLOOD, ETC"]
[null,"UTR","E","UNABLE TO REACH WELL",null,"ALL WEATHER RELATED REASONS PREVENTING LOCATION ACCESS - MUD, WASH OUT, FLOODED, SNOW DRIFTS, ETC"]
[null,"LTG","F","LIGHTNING STRIKE",null,"PROBLEMS WITH ACTUAL OR POTENTIAL LIGHTNING EVENTS AFFECTING OR DESTROYING EQUIPMENT"]
[null,"SUR","G","SURFACE EQUIPMENT FREEZE",null,"PROBLEMS WITH HYDRATES IN SURFACE PRODUCTION EQUIPMENT - WELLHEAD, CHOKE, SEPARATORS, ETC"]
[]
[null,null,"43  TOTAL  REASONS"]